

Working pressure: -1,0 / +1,0 Bar